Title: afgafgasdgfsd
Author: Bruce Ferguson
Last saved by: Michael Griffith
Company: None

Permit Review Summary
Page

PERMIT REVIEW SUMMARY

Permit Writer:	Michael Griffith			Date:	August 16, 2016

Company Name:	US Navy, Naval Construction Battalion Center

Facility Location:	5200 CBC
2nd Street Code 17
Gulfport, MS

Source Number:	1020-00080

County: 		Harrison

PROJECT DESCRIPTION AND LIMITATIONS

US Navy, NCBC is renewing their Synthetic Minor Operating Permit.  NCBC is requesting modifications to streamline and optimize the current operating permit requirements while providing operational flexibility for growth to meet military operational readiness.

Emission Point AA-001 contains all natural gas fired, external combustion units at the facility, is restricted to burning 300,000,000 cubic feet per consecutive 12-month period of natural gas, and is required to keep a log of all equipment on base included in this emission point.

Emission Point AA-002 contains all diesel fired, emergency backup internal combustion generators, fire pumps, and water pumps.  The facility has requested an increase to its total combined operating limit from 2,687,040 kW-hrs to 2,718,000 kW-hrs for all units and must keep a log of all equipment on base included in this emission point.  The facility is also limited to firing fuel oil with a maximum sulfur content of 0.5% Sulfur by weight and shall monitor and keep records of the fuel oil content of each fuel shipment received.  

Emission Point AA-003 contains the painting, cleaning, and solvent usage operations.  The facility is restricted to 50.0 Tons/year of VOCs, 9.0 Tons/year of Single HAPs, and 24.0 Tons/year of Total HAPs from this emission point.  The facility shall monitor the quantity, percentage of VOC by weight, percentage of each individual HAP and total HAP by weight, and the density for each coating, adhesive, solvent, or other VOC or HAP containing material used.  The following records shall be kept:  a)  Records of the identification of each coating, adhesive, solvent or other VOC or HAP containing material and the total gallons of each material used on a monthly basis and in each consecutive 12 month period.  b)  The VOC and HAP content of each coating, adhesive, solvent or other VOC or HAP containing material used.  c)  The density of each coating, adhesive, solvent, or other VOC or HAP containing material used. d)  The total VOC emission rate, the emission rate of each individual HAP and the total HAP emission rate in tons/year for each consecutive 12-month period.

Emission Point AA-004 contains all woodworking and carpentry operations.  The facility shall use cyclones for control of particulate matter.

Emission Point AA-005 contains all gasoline fueling operations and associated storage tanks.  The facility is restricted to 30.1 Tons/year of VOC emissions from this emission point.  This emission point is subject to and shall comply with the National Emission Standards for Hazardous Air Pollutants for Gasoline Dispensing Facilities and the General Provisions (40 CFR 63, Subpart CCCCCC and A) because it has a monthly throughput greater than 100,000 gallons of gasoline.  

Emission PoinAA-006 contains all welding activities at the facility.

Emission Point AA-008 contains various natural gas fired emergency backup internal combustion generators.  The facility is restricted to a total combined operating limit of 42,500 kW-hrs for all units and must keep a log of all equipment on base included in this emission point.

Emission Point AA-009 is a new emission point requested by the permittee.  This emission point consists of fire-fighting training operations.  The permittee has requested a limit of 160 wooden pallets and 500 gallons of propane burned.  The permittee shall keep records to document the number of wooden pallets used and total gallons of propane burned during any consecutive 12-month period. Records shall be kept on site for a period of not less than three years and made available to DEQ personnel upon request.

For Emission Points 002 and 008, NCBC is required to evaluate the applicability of the Standards of Performance for Stationary Compression Ignition Internal Combustion Engines (40 CFR 60, Subpart IIII), Standards of Performance for Stationary Spark Ignition Internal Combustion Engines (40 CFR 60, Subpart JJJJ), and National Emission Standards for Hazardous Air Pollutants for Reciprocating Internal Combustion Engines (40 CFR 63, Subpart ZZZZ).  NCBC shall comply with all applicable standards for any engine subject to these regulations. 

For Emission Point AA-001, NCBC is not subject to the National Emission Standards for Hazardous Air Pollutants for Area Sources:  Industrial, Commercial, and Institutional Boilers (40 CFR 63, Subpart JJJJJ).  NCBC only has boilers with a rated capacity of less than 9.9 MMBTU/hr and they only burn natural gas.

Emissions Summary
Pollutant | lb/hr | tpy
Carbon Monoxide | 107.86 | 28.92
Nitrogen Oxides | 478.82 | 90.74
Sulfur Dioxide | 30.94 | 5.04
Particulate Matter | 37.79 | 18.27
Volatile Organic Compounds | 60.94 | 89.23
Total Hazardous Air Pollutants | 3.00 | 10.86

PUBLIC PARTICIPATION

The 30-day public notice period began on August 16, 2016, with the publication of a notice in the Sun Herald and ends September 15, 2016.

RECOMMENDATION

The staff has preliminarily decided to recommend issuance of the permit to the Mississippi Environmental Quality Permit Board as shown in the draft permit.  However, the staff recommendation to the Board will be made only after a thorough consideration of all public comments.

3290 PER20160001