PRETREATMENT RATIONALE FOR ISSUANCE

Niagara Bottling LLC
Marshall County
Byhalia, MS
Agricultural Branch

MSP092402
SIC: 2086
April 4, 2017
Permit Engineer: Joe McNamara

I.	FACILITY INFORMATION

A.	Nature of Business: Manufacture bottled water
B.	Process Wastewater Description: Process related wastewater, non-contact cooling water
C.	Proposed Flowrate: 0.3 MGD
D.	Applicable Federal Guidelines: 40 CFR Part 403 General Pretreatment

II.	RECEIVING POTW INFORMATION

A.	POTW and Permit Number: Marshall Utility Services LLC, Chickasaw Trail Wastewater Treatment Plant  (MS0060046 AI:22256)
B.	POTW Treatment Type: Activated Sludge followed by Ultraviolet Disinfection 
C.	POTW Design Flowrate: NPDES Permit No. MS0060046 is currently being modified for a flow increase to 1.0 MGD over three Phases.  Upon issuance of this permit, compliance shall be achieved with the Phase I flow limit (0.15 MGD).  Beginning upon completion and start-up of improvements to increase the wastewater treatment facility’s design flow rate to 0.45 MGD, compliance shall be achieved with the Phase II flow limit (0.45 MGD).  Beginning upon completion and start-up of improvements to increase the wastewater treatment facility’s design flow rate to 1.0 MGD, compliance shall be achieved with the Phase III flow limit (1.0 MGD).
D.	POTW Receiving Stream (7Q10): Coldwater River (1.3 cfs)
E.	POTW 12-month Average Flowrate: 0.056 MGD

III.	APPLICATION DATA

Parameter	Daily Max	Parameter	Daily Max	
BOD5	24 mg/L	Bromide	169.2 mg/L	
COD	102.4 mg/L	Fluoride	169.2 mg/L	
TSS	17.8 mg/L	Nitrate-Nitrite	169.2 mg/L	
pH	6.0 – 9.0 S.U.	Sulfate	169.2 mg/L	

IV.	LIMITATION  RECOMMENDATIONS  FROM  POTW

Parameter	Daily Max	Parameter	Daily Max	
BOD5	Report	Bromide	Report	
Flow	0.30 MGD	Fluoride	Report	
TSS	Report	Nitrate-Nitrite	Report	
pH	6.0 – 9.0 S.U.	Sulfate	Report	

V.	PROPOSED PERMIT LIMITATIONS (OUTFALL 001)
		
Parameter	Daily Max	Monthly Average	
BOD5	Report mg/L, lbs/day	Report mg/L, lbs/day	
TSS	Report mg/L, lbs/day	Report mg/L, lbs/day	
Flow	0.3 MGD	Report MGD	
pH	9.0 S.U. 	6.0 S.U. (min)	

BOD5 and TSS shall be monitored twice per month with 24-hr composite sample.  Flow shall be monitored daily with a continuous recorder.  pH shall be monitored daily with a grab sample.

For the first one hundred eighty (180) days after the commencement of discharge, the permittee shall monitor Ammonia Nitrogen and all pollutants listed in Parts B and C of Form 2P twice per month with a 24-hour composite sample.  Data shall be submitted in a monthly report to Marshall Utility Services LLC, Chickasaw Trail Wastewater Treatment Plant at the following address:
520 J M Ash Drive
Holly Springs MS, 38635.

Within one hundred eighty (180) days after the commencement of discharge, the permittee shall submit a completed Pretreatment Form 2P application and a summary of monthly reports required by Permit Condition S-1.  Based upon the results of analyses, the permit may be reopened and reissued to reflect this data.