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INFORMATION RELATIVE TO 
THE DRAFT TITLE V OPERATING PERMIT
August 17, 2026

GENERAL FACILITY INFORMATION
Facility Name:  Tishomingo Acquisition LLC, dba TBEI, Tishomingo
Facility Address:  1425 Highway 25 North; Tishomingo, MS  38873  
1425 Highway 25 North
County: Tishomingo
SIC Code(s): 3713, 3715
NAICS Code(s): 336211  

APPLICATION SUMMARY 
	Permit No.: 2640-00002
Permit Action:  Renewal 
Permit Folder: PER20260001
Application Receipt Date: 04/16/2026
Application Deemed Complete: 07/15/2026
CBI Submitted?: No
	NSPS (Part 60): N/A
NESHAP (Part 61): N/A
NESHAP (Part 63): Subpart MMMM 
112(r) / RMP: N/A
Other: N/A



FACILITY DESCRIPTION
Tishomingo Acquisition, LLC (d.b.a. TBEI – Tishomingo) is an existing manufacturer of truck dump bodies and hoists.  The facility’s operations fall under SIC Codes 3713 (Truck and Bus Bodies) and 3715 (Truck Trailers) and North American Industry Classification System (NAICS) Codes 336211 (Motor Vehicle Body Manufacturing). 

Operations begin with carbon, stainless steel, and aluminum sheets conveyed to series of metalworking activities (such as shearing, cutting, drilling, pressing and welding).  The metal components then undergo grinding, abrasive blasting, and phosphatizing prior to surface coating in one of three (3) spray booths. The space heaters, heaters for drying the metal components, metalworking activities (brushing, cleaning, drilling, grinding, pressing, sanding, scraping and welding), phosphatizing activities, and storage tanks are classified as “insignificant activities”. 

TITLE V SOURCE APPLICABILITY 
The facility’s potential-to-emit (PTE) exceeds the Title V major source threshold of 100 tons per year (tpy) for volatile organic compounds (VOCs) and particulate matter (PM).  Additionally, the facility’s potential-to-emit hazardous air pollutants (HAPs) exceeds the Title V major source thresholds of 25 tpy for total HAPs and 10 tpy for the following individual HAPs: ethyl benzene, xylene, toluene, methyl isobutyl ketone, methanol and glycol ethers.  Hence, the facility is a major source for HAPs. 

Facility-Wide Potential-to-Emit Summary1
	Pollutant
	PTE Emissions
(tons/yr)

	Particulate Matter (TSP)
	98.812

	PM10
	98.812

	PM2.5
	98.812

	Sulfur Dioxide (SO2)
	1.19

	Nitrogen Oxides (NOx)
	25.68

	Carbon Monoxide (CO)
	10.65

	Volatile Organic Compounds (VOC)
	240.0

	Total HAP 
	240.0


1 The PTE emissions reflect any emission limits or enforceable restrictions included in the proposed permit.
2 The PTE of PM is greater than the Title V threshold of 100 tpy; however, many of the PM emitting devices are equipped with inherent dust collectors that reduce these emissions (“inherent process equipment” means equipment that is necessary for the proper and safe functioning of the process, or material recovery equipment that the is installed and operated primarily for purposes other than compliance with air pollution regulations).

PREVENTION OF SIGNIFICANT DETERIORATION (PSD) APPLICABILITY
The facility is not one (1) of the 28 categorical facilities listed in 40 CFR 52.21(b)(1)(i)(a); therefore, the PSD threshold for a major source is 250 tpy.  The facility has the potential to emit more than 250 tpy of total particulate matter (PM), PM less than 10 microns (µm) in diameter (PM10), PM less than 2.5 µm in diameter (PM2.5), and VOC.  To avoid PSD major source status for PM, the facility will not bypass the air emission control devices (i.e. dust collectors and filters) while the corresponding process equipment is in operation.  For VOC, the facility will monitor and record VOC emitting material used at the site.  Therefore, the facility is considered a moderate stationary source.

FACILITY MODIFICATIONS AND/OR PERMIT CHANGES
Upon review of the submitted application, the MDEQ has incorporated the following modifications:

· Facility installed one Bystronic laser cutting machine (Emission Point AA-011), which is equipped with cartridge dust collector to control particulate matter (PM/PM10) emissions.  This equipment has been added to Condition 3.B.3 to prohibit bypassing the dust collector as well as Condition 5.B.2 for monthly inspection.
· The facility submitted three (3) 502(b)(10) change requests since the previous reissuance.  These changes included replacement of the Finish Paint Booth #1 and Parts Paint Booth.  These changes did not result in an increase of emissions or require new permit limitations.

COMPLIANCE ASSURANCE MONITORING (CAM) APPLICABILITY
40 CFR Part 64 specifies the requirements for CAM.  The general applicability of this rule can be found in 40 CFR 64.2 and requires a Title V source to comply with the CAM requirements if all three of the following criteria are met for a pollutant-specific emission unit (PSEU):

1. The unit is subject to an emission limitation or standard for a regulated air pollutant other than exemptions under 40 CFR 64.2(b)(1);
2. The unit uses a control device to comply with the standard; and
3. The unit has pre-control emissions exceeding Title V major source threshold.

CAM Applicability Table for Sources with Control Devices
	Emission Point ID
	Control Device 
(not including inherent controls)
	Applicable Limit/ Standard
	Is standard exempt? (Yes/No)
	Pre-Control > 100 tpy (Yes/No)
	CAM Applies? (Yes/No)
	Type of CAM PSEU
(Large/Other)

	AA-009
	Four (4) Dry Filters
	PM Process Weight
	No
	No
	No
	N/A

	AA-010a
	One (1) Dust Collector
	PM Process Weight
	No
	Yes
	Yes
	Other

	AA-010b
	Two (2) Dust Collectors
	PM Process Weight
	No
	No
	No
	N/A

	AA-011
	One (1) Dust Collector
	PM Process Weight
	No
	No
	No
	N/A



· The maximum uncontrolled emissions from Emission Point AA-009, AA-010b and AA-011 is 98.83 tpy, 21.00 tpy, and 27.81 tpy, respectively.  

· Potential uncontrolled emissions of PM from Emission Point AA-010a (286.65 tpy) exceed the major source threshold. The blast booth is limited by a facility wide PM limit (the process weight equation which is a proxy for PM2.5 and PM10 emissions), uses a control device to achieve compliance, and is not otherwise exempt.


NATIONAL EMISSION STANDARDS FOR HAZARDOUS AIR POLLUTANTS (NESHAP) APPLICABILITY

40 CFR Part 63, Subpart MMMM – National Emission Standards for Hazardous Air Pollutants for Surface Coating of Miscellaneous Metal Parts and Products:  This subpart applies to facilities that are major sources of HAPs and use more than 250 gallons per year of HAP-containing materials in the surface coating of miscellaneous metal parts and products.  Tishomingo Acquisition, LLC is subject to the requirements of this subpart as it is a major source of HAP that uses more than 250 gallons per year of HAP containing material coating motor vehicle parts and accessories.  Moreover, the facility is considered an existing general use coating affected source (commenced constriction prior to August 13, 2002) and is limited to 2.6 pounds of organic HAPs per gallon of coating solids used in a rolling 12-month period.  Currently, the facility demonstrates compliance with this limit using the “Emission Rate Without Add-on Controls Option.” The “Compliant Material Option” was previously incorporated into the permit as an alternative compliance option and remains in this draft.

40 CFR Part 63, Subpart IIII, National Emission Standards for Hazardous Air Pollutants for Surface Coating of Automobiles and Light-Duty Trucks:	This subpart applies to any facility that is major source of HAPs and performs surface coating on automobiles and light-duty trucks and/or their components (with gross vehicle weight rating of 8,500 pounds or less). Tishomingo Acquisition, LLC constructs bodies for dump trucks, which weigh over 15,000 pounds.  Therefore, this subpart is not applicable.

40 CFR Part 63, Subpart PPPP—National Emission Standards for Hazardous Air Pollutants for Surface Coating of Plastic Parts and Products:	This subpart establishes national emission standards for hazardous air pollutants (NESHAP) for plastic parts and products surface coating facilities. This subpart also establishes requirements to demonstrate initial and continuous compliance with the emission limitations. Tishomingo Acquisition, LLC operates a metal coating operation.  Therefore, this subpart is not applicable.
	
40 CFR Part 63, Subpart HHHHHH—National Emission Standards for Hazardous Air Pollutants: Paint Stripping and Miscellaneous Surface Coating Operations at Area Sources:  This subpart establishes national emission standards for hazardous air pollutants (HAP) for area sources involved in activities such as paint stripping, autobody refinishing operations, and spray painting of target HAPs.  Tishomingo Acquisition, LLC is considered a major source of HAP; therefore, the facility is not subject to the provisions of Subpart HHHHHH.

NEW SOURCE PERFORMANCE STANDARDS (NSPS) APPLICABILITY

40 CFR Part 60, Subpart MM—Standards of Performance for Automobile and Light Duty Truck Surface Coating Operations for which Construction, Modification or Reconstruction Commenced After October 5, 1979, and On or Before May 18, 2022:	The provisions of this subpart apply to the facilities in an automobile or light-duty truck assembly plant: each prime coat operation, each guide coat operation, and each topcoat operation.  Tishomingo Acquisition, LLC constructs bodies for dump trucks, which weigh over 15,000 pounds.  Therefore, this subpart is not applicable.  

40 CFR Part 60, Subpart MMa—Standards of Performance for Automobile and Light Duty Truck Surface Coating Operations for which Construction, Modification or Reconstruction Commenced After May 18, 2022:	The provisions of this subpart apply to the facilities in an automobile or light-duty truck assembly plant.  Tishomingo Acquisition, LLC constructs bodies for dump trucks, which weigh over 15,000 pounds.  Therefore, this subpart is not applicable.    

SPECIFIC APPLICABLE REQUIREMENTS

	Emission Point No.
	Pollutant
	Draft Permit Emission Limits
	Monitoring Requirements

	AA-000
(Facility-Wide)
	Opacity
	40%
	The facility is expected to show a significant margin of compliance; therefore, no monitoring is required.

	
	PM
(filterable)
	E = 4.1 (p0.67)
	Daily visible emission observations, which may result in visible emissions evaluations (VEEs) and weekly inspections on the air pollution control equipment for AA-010a as outlined in the CAM Plan.

	
	VOCs
	240.0 tpy

(Rolling 12-Month Total)
	Calculate and record the emission of VOCs (monthly & rolling 12-month totals)

	AA-009
	Organic HAPs
	2.6 Pounds per Gallon Coating Solids during Each 12-month Compliance Period
	Compliant Material Option: Demonstrate that the organic HAP content of each coating is less than or equal to the emission limit and that each thinner and/or other additive, and cleaning material used contains no organic HAPs.

Emission Rate without Add-on Controls Option: Demonstrate that, based on the coatings, thinners and/or other additives, and cleaning materials used, the organic HAP emission rate for the coating operation(s) is less than or equal to the emission  limit, calculated as a rolling 12-month emission rate and determined on a monthly basis.

	AA-009
AA-010a
AA-010b
AA-011
	PM / PM10
	No Bypass of Air Pollution Control Equipment

(PSD Avoidance Limits)
	Operate and conduct inspections on the air pollution control equipment on a weekly basis for AA-010a and monthly basis for AA-009, AA-010b, AA-011.
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