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INFORMATION RELATIVE TO 
THE DRAFT TITLE V OPERATING PERMIT
September 4, 2026

GENERAL FACILITY INFORMATION
Facility Name:  BlueScope Coated Products LLC
Facility Address:  
951 Prisock Road
Jackson, MS 39272    
County: Hinds
SIC Code(s): 3479 (Coatings, Engravings, and Allied Services)
NAICS Code(s): 332812 (Metal Coating, Engraving (except Jewelry and Silverware), and Allied Services to Manufacturers)

APPLICATION SUMMARY 
	Permit No.: 1080-00068
Permit Action: Renewal 
Permit Folder: PER20250001
Application Receipt Date: January 31, 2025
Application Deemed Complete: August 8, 2026
CBI Submitted?: No
	NSPS (Part 60): A, TT
NESHAP (Part 61): N/A
NESHAP (Part 63): A, SSSS
112(r) / RMP: N/A
Other: N/A



FACILITY DESCRIPTION
BlueScope Coated Products is an existing metal coil coating facility.  The process includes cleaning, pre-treatment, and surface coating of rolled (coiled) sheet metal on a single continuous coating line (Emission Point AA-001).  The facility also operates a 10,000-gallon virgin solvent storage tank (Emission Point AA-002).  The surface coating operation is equipped with an emissions captures system routed to a 46 million BTU (MMBTU) per hour natural gas-fired thermal oxidizer for the destruction of volatile organic compounds (VOC).  Insignificant activities at the site include space and infrared heaters, maintenance equipment, and small storage tanks.

TITLE V SOURCE APPLICABILITY 
The facility’s potential-to-emit (PTE) exceeds the Title V major source threshold of 100 tons per year (tpy) for each of the following criteria air pollutants: Volatile Organic Compounds (VOC).  The facility’s potential-to-emit hazardous air pollutants (HAPs) exceeds the Title V major source thresholds of 25 tpy of total HAPs and 10 tpy for the following individual HAPs: Xylenes (mixed isomers).

Facility-Wide Potential-to-Emit Summary1
	Pollutant
	PTE Emissions
(tpy)

	Particulate Matter (TSP)
	1.49

	PM10
	1.49

	PM2.5
	1.49

	Sulfur Dioxide (SO2)
	0.13

	Nitrogen Oxides (NOx)
	19.62

	Carbon Monoxide (CO)
	16.51

	Volatile Organic Compounds (VOC)
	240.01

	Total HAP 
	50.11


1 The PTE emissions reflect any emission limits or enforceable restrictions included in the proposed permit.

PREVENTION OF SIGNIFICANT DETERIORATION (PSD) APPLICABILITY
The facility is not one of the 28 categorical facilities listed in 40 CFR 52.21(b)(1)(i)(a); therefore, the PSD threshold for a major source is 250 tpy.  The facility has the potential-to-emit more than 250 tons per year of VOC but will continue to limit facility-wide emissions of VOC to 240.0 tpy; therefore, the facility is considered a moderate stationary source. This permitting action will not change the current PSD status of the facility.

FACILITY MODIFICATIONS AND/OR PERMIT CHANGES
The facility has not proposed any changes during this permitting action.  Minor administrative changes to the permit were incorporated through this permitting action, such was addition of the state regulation for particulate matter (PM) for manufacturing processes and correcting various references.

COMPLIANCE ASSURANCE MONITORING (CAM) APPLICABILITY
40 CFR Part 64 specifies the requirements for CAM.  The general applicability of this rule can be found in 40 CFR 64.2 and requires a Title V source to comply with the CAM requirements if all three of the following criteria are met for a pollutant-specific emission unit (PSEU):

1. The unit is subject to an emission limitation or standard for a regulated air pollutant other than exemptions under 40 CFR 64.2(b)(1);
2. The unit uses a control device to comply with the standard; and
3. The unit has pre-control emissions exceeding Title V major source threshold.

The Continuous Coil Coating Line (Emission Point AA-001) has a pre-control emission rate of VOC greater than the Title V threshold of 100 tons per year.  It also is subject to an emission limit for VOC and utilizes a thermal oxidizer to control these emissions.  Therefore, CAM does apply to this unit.  Because the post-control emissions are proposed to exceed the major source threshold, it is considered a “large” PSEU.  No changes to the existing CAM plan were requested through this permitting action.  

CAM Applicability Table for Sources with Control Devices
	Emission Point ID
	Control Device 
(not including inherent controls)
	Applicable Limit/ Standard
	Is standard exempt? (Yes/No)
	Pre-Control > 100 tpy (Yes/No)
	CAM Applies? (Yes/No)
	Type of CAM PSEU
(Large/Other)

	AA-001
	Thermal Oxidizer
	≤ 240 tpy
	No
	Yes
	Yes
	Large



NATIONAL EMISSION STANDARDS FOR HAZARDOUS AIR POLLUTANTS (NESHAP) APPLICABILITY

40 CFR 63, Subpart XXXXXX – National Emission Standards for Hazardous Air Pollutants Area Source Standards for Nine Metal Fabrication and Finishing Source Categories: this subpart applies to area sources that engage in nine specific industry sectors.  This facility is a major source of HAPs; therefore, the subpart does not apply.

40 CFR 63, Subpart MMMM – National Emission Standards for Hazardous Air Pollutants for Surface Coating of Miscellaneous Metal Parts and Products: this subpart applies to coating miscellaneous metal parts.  The subpart specifies in 40 CFR 63.3881(c)(14) that facilities subpart to the metal coating requirements of 40 CFR 63, Subpart SSSS, are not subject to the requirements of this subpart; therefore, the subpart does not apply.

40 CFR 63, Subpart HHHHHH – National Emission Standards for Hazardous Air Pollutants: Paint Stripping and Miscellaneous Surface Coating Operations at Area Sources: this subpart applies to paint stripping, autobody refinishing, and spray application of coatings with target HAP operations at area sources.  This facility is a major source; therefore, the subpart does not apply.

40 CFR 63, Subpart SSSS – National Emission Standards for Hazardous Air Pollutants: Surface Coating of Metal Coil: this subpart applies to facilities that perform metal coil surface coating operations and are major sources of HAPs.  This facility performs metal coil coating and is a major source of HAP; therefore, this subpart does apply.  The subpart requires the facility meet an organic HAP emission limit by operating a thermal oxidizer and capture system on the coil coating process.  The facility will demonstrate compliance with periodic performance testing and measuring the temperature in the thermal oxidizer combustion chamber.

NEW SOURCE PERFORMANCE STANDARDS (NSPS) APPLICABILITY

40 CFR 60, Subpart TT – Standards of Performance for Metal Coil Surface Coating: this subpart applies to metal coil surface coating operations.  This facility operates a metal coil coating line; therefore, this subpart applies.  The coil coating process is subject to a VOC emission limit and will demonstrate compliance through emissions calculations and continuously monitoring the thermal oxidizer.

SPECIFIC APPLICABLE REQUIREMENTS

	Emission Point(s)
	Pollutant/ Parameter
	Limit/Standard
	Monitoring Requirements

	AA-001
	VOC
	≤ 240.0 tpy
	Permittee must track all VOC/HAP containing material used at the site, conduct performance testing on the thermal oxidizer, and monitor performance including Compliance Assurance Monitoring requirements

	
	PM (filterable)
	E = 4.1 × p0.67
	Margin of compliance is large; no monitoring proposed.

	
	
	E = 0.8808 × I-0.1667
	

	
	SO2
	≤ 4.8 lb/MMBTU
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