PERMIT RATIONALE FOR REISSUANCE
Mike Alderson, Mike Alderson Duplexes
Lafayette County
Oxford, Mississippi
Water SOP No. MSU030187
March 2017

I.	CLASSIFICATION – Commercial State Operating Permit (SOP)

II.	DESCRIPTION OF WASTEWATER – Domestic Wastewater

III.	DESCRIPTION OF WASTEWATER TREATMENT - Wastewater treated by means of aerated treatment units (ATU’s), and the effluent is distributed to gravel disposal systems. Maximum design flow is 2000 gallons per day.

IV.	RECEIVING WATERS – None, no discharge to surface waters is described in the application.

V.	APPLICABLE GUIDELINES – 11 Mississippi Admin Code pt. 6

VI.	SUMMARY OF LIMITATIONS – None, no discharge to surface waters is described in the application.

The wastewater treatment and disposal system for this project must protect water quality. This permit is subject to modification if future evidence, monitoring results, or other information indicates that surface water quality is being adversely affected.  This permit may be modified to require monitoring of surface water if needed to ensure that water quality is being protected.

Operation of the wastewater treatment and disposal system for this project shall cease and connection made to a regional or municipal sewer system when available in the area.