PERMIT RATIONALE FOR REISSUANCE
Mr. Jiffy Inc
Panola County
Batesville, Mississippi
Water NPDES No. MS0058807
June 2017

I.	FACILITY INFORMATION

Facility Name:  	Mr. Jiffy Inc
Facility Address:  	1188 Highway 6 East 
	Batesville, MS  38606    
Batesville, 
Permit No.:  		MS0058807
SIC: 	 		7542
Permit Writer:  	Haley Sims
EPD Branch:  		Service and Miscellaneous Industries Branch

II.	NATURE OF BUSINESS

Mr. Jiffy Inc. operates a convenient store and car wash in Batesville, MS. 

III.	EFFLUENT AND RECEIVING STREAM FLOW DATA

The application details an effluent of 1,000 gpd of treated carwash waste water discharged to an unnamed creek thence into the Tallahatchie River.

IV.	303(d) ISSUES

None.
A TMDL has been developed for the Tallahatchie River, where the pollutants of concern are organic enrichment, low DO, Sediment, and siltation. 

V.	TYPE OF WASTEWATER TREATMENT

Oil/water separator and sedimentation.

VI.	EPA APPLICABLE CATEGORICAL GUIDELINES

None. 

VII.	DATA FROM APPLICATION FORM (Short Form D)

Parameter	Maximum Daily Value	
Flow	1,000 gpd	

VIII. 	WATER QUALITY LIMITATIONS BASED ON WASTELOAD ALLOCATION 

	Not Applicable. 

IX.	CATEGORICAL GUIDELINE LIMITATIONS CALCULATIONS

Not Applicable. 

X.	TOXICITY SCREENING

Not Applicable.

XI.	PROPOSED FINAL LIMITATIONS 

1.	Average Permit Limitations

Outfall	Parameter	Categorical Limitation	Water Quality Limitation	Present Permit Limitation	Proposed Permit Limitation	Basis	
MS0058807-001	Flow 	N/A	N/A	1,600 gpd	1,000 gpd	APP	
MS0058807-001	TSS	N/A	N/A	30 mg/L	30 mg/L	PPL	
MS0058807-001	Oil & Grease	N/A	N/A	10 mg/L 	10 mg/L	PPL	
MS0058807-001	pH	N/A	N/A	6.0 < pH < 9.0 s.u. 	6.0 < pH < 9.0 s.u.	PPL	
PPL = Previous Permit Limit 
APP = Application Form (Short Form D) 

2.	Maximum Permit Limitations

Outfall	Parameter	Categorical Limitation	Water Quality Limitation	Present Permit Limitation	Proposed Permit Limitation	Basis	
MS0058807-001	Flow 	N/A	N/A	1,600 gpd	1,000 gpd	APP	
MS0058807-001	TSS	N/A	N/A	45 mg/L	45 mg/L	PPL	
MS0058807-001	Oil & Grease	N/A	N/A	15 mg/L 	15 mg/L	PPL	
MS0058807-001	pH	N/A	N/A	6.0 < pH < 9.0 s.u. 	6.0 < pH < 9.0 s.u.	PPL	
PPL = Previous Permit Limit
APP = Application Form (Short Form D)
There is currently no monitoring required for this permitted discharge. The effluent limits for the discharge have been developed such that the waste treatment system should protect the water quality.  However, this permit is subject to modification if future evidence, monitoring results, or nuisance conditions indicate a higher degree of treatment is required to maintain water quality in the receiving stream.