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INFORMATION RELATIVE TO 
THE TITLE V OPERATING PERMIT
July 6, 2026

GENERAL FACILITY INFORMATION
Facility Name:  City of Canton, Canton Sanitary Landfill
Facility Address:  303 Soldier Colony Road; Canton, MS 39046
County: Madison
SIC Code(s): 4953 – Refuse Systems
NAICS Code(s): 562212 – Solid Waste Landfill

APPLICATION SUMMARY 
	Permit No.: 1780-00080
Permit Action:  Initial Issuance 
Permit Folder: PER20220002
Application Receipt Date: 01/14/2022
Application Deemed Complete: 08/17/2022
CBI Submitted?  No
	NSPS (Part 60): Subpart XXX* 
NESHAP (Part 61): N/A
Federal Plan (Part 62): Subpart OOO*
NESHAP (Part 63): N/A
112(r) / RMP: N/A
Other: N/A


*	The facility is subject to 40 CFR 62, Subpart OOO until such time the facility commences construction of the proposed lateral expansion.  Once construction begins, the facility will be subject to 40 CFR Part 60, Subpart XXX and longer subject to 40 CFR Part 62, Subpart OOO.  

FACILITY DESCRIPTION
The City of Canton – Canton Sanitary Landfill (“Canton Landfill”) is an existing municipal solid waste (MSW) landfill that is owned by the City of Canton and has been in operation since 1986.  Currently, the landfill has a permitted design capacity of 1,332,505 tons; however, the facility has submitted an application requesting an initial Title V Operating Permit (TVOP) to reflect a proposed expansion of the landfill that will result in an increased design capacity of 3,940,031 tons (or 3,574,337 metric tons) and 6,566,719 cubic yards (or 5.02 million cubic meters)

Based on the application, Canton Landfill will accept non-hazardous solid waste from residential, industrial, and institutional sources (which includes – but not limited to – household waste, commercial waste, and industrial waste, rubbish, construction debris, and non-asbestos-containing demolition material).  Waste materials are transported by mobile equipment, which causes fugitive dust emissions.  The mobile equipment is fueled by two (2) on-site diesel storage tanks.


TITLE V SOURCE APPLICABILITY 
Under current operations, Canton Landfill’s design capacity is less than 2.5 million megagrams and 2.5 million cubic meters.  As such, the facility was not required to obtain a TVOP.  However, upon issuance of the proposed TVOP (in tandem with the proposed modification of the State of Mississippi Solid Waste Management Permit No. SW04501B0378 issued November 14, 2017), the facility will have the authority to enact a proposed lateral expansion of the landfill.  Upon commencing construction of the proposed expansion, Canton Landfill will have a design capacity greater than 2.5 million megagrams and 2.5 million cubic meters.  Therefore, pursuant to 40 CFR Part 60 – Subpart XXX [specifically 40 CFR 60.762(b) and (c)], Canton Landfill is required to obtain a TVOP.
Regarding air emissions, the facility’s potential-to-emit (PTE) does not the Title V major source threshold of 100 tons per year (tpy) for any of the applicable criteria air pollutants.  In addition, the facility’s potential-to-emit hazardous air pollutants (HAPs) does not exceed the major source threshold of 25 tons per year for all HAPs in total or 10 tons per year for each individual HAP.  Therefore, the facility is considered an area source for HAPs.
Facility-Wide Potential-to-Emit Summary1
	Pollutant
	PTE Emissions
(tons/yr)

	Particulate Matter (TSP)
	8.86

	PM10
	8.86

	PM2.5
	0.29

	Sulfur Dioxide (SO2)
	0.00

	Nitrogen Oxides (NOX)
	0.00

	Carbon Monoxide (CO)
	1.98

	Volatile Organic Compounds (VOCs)
	16.38

	Total Reduced Sulfur (TRS)
	0.00

	Lead
	0.00

	CFC/HCFC
	1.035

	Total HAPs
	13.41


1	The PTE emissions reflect any emission limits or enforceable restrictions included in the proposed permit and are based on the emissions after the lateral expansion of the landfill.

PREVENTION OF SIGNIFICANT DETERIORATION (PSD) APPLICABILITY
A MSW landfill is not one of the 28 categorical facilities listed in 40 CFR 52.21(b)(1)(i)(A); therefore, the applicable PSD major source threshold is 250 tons per year for each regulated New Source Review (NSR) pollutant (with fugitive emissions not included in the initial assessment).  Based on the emissions profile, Canton Landfill does not have the potential to emit any regulated pollutant more than 250 tons per year.  Therefore, the facility is considered an existing “minor NSR source” under the PSD program. 
This permitting action will not change the current PSD status of the facility.
FACILITY MODIFICATIONS AND/OR PERMIT CHANGES
As discussed previously, a lateral expansion of the landfill was addressed in the Title V application to increase the waste disposal capacity from 1,332,505 tons to 3,940,031 tons.  Prior to the expansion, the facility is subject to the requirements of 40 CFR 62, Subpart OOO – Federal Plan Requirements for Municipal Solid Waste Landfills That Commenced Construction On or Before July 17, 2014 and Have Not Been Modified or Reconstructed Since July 17, 2014.  Since the design capacity was less than 2.5 million megagrams per year and 2.5 million cubic yards, the facility was only required to submit the initial design capacity report until such time the landfill is modified to exceed these thresholds. 

Since the facility is proposing to expand the landfill after 2014 and the expansion will result in the capacity thresholds being exceeded, the facility will be subject to the applicable requirements of 40 CFR Part 60, Subpart XXX instead of 40 CFR Part 62 Subpart OOO.  The emissions from the landfill are not required to be collected and controlled given that the estimated emission rate of non-methane organic compounds (NMOCS) does not exceed the regulatory threshold (i.e., 34 megagrams per year).  Once the estimated NMOC emission rate exceeds the referenced threshold, Canton Landfill will be required to design, install, and operate a gas collection and control system (GCCS). 

COMPLIANCE ASSURANCE MONITORING (CAM) APPLICABILITY
40 CFR Part 64 specifies the requirements for CAM.  The general applicability of this rule can be found in 40 CFR 64.2 and requires a Title V source to comply with the CAM requirements if all three of the following criteria are met for a pollutant-specific emission unit (PSEU):
1. The unit is subject to an emission limitation or standard for a regulated air pollutant other than exemptions under 40 CFR 64.2(b)(1);
2. The unit uses a control device to comply with the standard; and
3. The unit has pre-control emissions exceeding Title V major source threshold.
As the MSW landfill (i.e., the PSEU) is not subject to an emission limit that meets the indicated criteria nor is there any control equipment associated with the landfill, CAM is not applicable.

NATIONAL EMISSION STANDARDS FOR HAZARDOUS AIR POLLUTANTS (NESHAP) APPLICABILITY
40 CFR Part 61, Subpart M – NESHAP: National Emission Standards for Asbestos: The provisions of Subpart M are applicable to an active waste disposal site that receives asbestos-containing materials for final disposal from sources also applicable to Subpart M.  As Canton Landfill has stated that it does not accept asbestos-containing waste, the facility is not subject to the provisions of Subpart M.

40 CFR Part 63, Subpart AAAA – NESHAP for Municipal Solid Waste Landfills: The provisions of Subpart AAAA are applicable to any municipal solid waste (MSW) landfill that has accepted waste since November 8, 1987, or has additional capacity for waste deposition and meets any one of the three following criteria:
1. The MSW landfill is a major source of HAP as defined in 40 CFR 63.2;
1. The MSW landfill is collocated with a major source as defined in 40 CFR 63.2; or
1. The MSW landfill is an area source that has a design capacity equal to or greater than 2.5 Mg and 2.5 million cubic meters and has estimated uncontrolled emissions equal to or greater than 50 megagrams of NMOCS per year.
Given that Canton Landfill does not have the capability to meet any of the referenced criteria (either in its current operations or after the enactment of the proposed lateral expansion), the facility is not subject to the provisions of Subpart AAAA.  

However, as 40 CFR Part 60 – Subpart XXX [specifically 40 CFR 60.762(b)(iv)] allows Canton Landfill to comply with specific provisions found in Subpart AAAA (40 CFR 63.1958, 63.1960, and 63.1961) in lieu of Subpart XXX (40 CFR 60.763, 60.765, and 60.766), the facility may opt to become subject to Subpart AAAA once it is required to commence operation of a GCCS pursuant to Subpart XXX.  If Canton Landfill chooses to comply with Subpart AAAA, the facility must continue operating the GCCS in accordance with Subpart AAAA and cannot return to the provisions of Subpart XXX.  

Should Canton Landfill choose to comply with Subpart AAAA in lieu of Subpart XXX), MDEQ only considers the facility subject to Subpart AAAA provisions explicitly cited in Subpart XXX (for applicability purposes).

NEW SOURCE PERFORMANCE STANDARDS (NSPS) APPLICABILITY
40 CFR Part 60, Subpart Cf – Emission Guidelines for Municipal Solid Waste Landfills: The provisions of Subpart Cf apply to any MSW landfill that commenced construction, modification, or reconstruction on or before July 17, 2014.  However, as an “emissions guideline”, a facility only becomes subject to Subpart Cf once the applicable environmental permit regulatory authority receives delegated authority through EPA’s approval of a State Plan completed in accordance with 40 CFR Part 60, Subpart Ba (Adoption and Submittal of State Plans for Designated Facilities).  
While MDEQ has not received delegated authority of Subpart Cf, it is MDEQ’s understanding that Canton Landfill will commence construction of the proposed expansion upon issuance of the renewed TVOP (in tandem with the modified Solid Waste Management Permit).  As construction of the denoted expansion will be considered a “modification” (as defined by 40 CFR Part 60, Subpart XXX), Canton Landfill will not be subject to Subpart Cf.
40 CFR Part 60, Subpart XXX – Standards of Performance for Municipal Solid Waste Landfills that Commenced Construction, Reconstruction, or Modification After July 17, 2014: The provisions of Subpart XXX are applicable to any solid waste landfill that commences construction, reconstruction, or modification after July 17, 2014.  While Canton Landfill was constructed prior to the denoted “effective date” of Subpart XXX the proposed lateral expansion will trigger the facility’s applicability to Subpart XXX because it will meet the definition of a “modification”.  
Pursuant to Subpart XXX, a modification is defined as the following: “an increase in the permitted volume design capacity of the landfill by either lateral or vertical expansion based on its permitted design capacity as of July 17, 2014.  Modification does not occur until the owner or operator commences construction on the lateral or vertical expansion.” 
Therefore, the provisions of Subpart XXX will be applicable once the facility commences construction on the expansion.  A “Tier 2” test conducted in 2018 resulted in the calculated NMOC emission rate of 11.4 megagrams per year.  As such, the facility is not required to design, install, and operate a GCCS at this time.
FEDERAL PLAN
40 CFR 62, Part Subpart OOO – Federal Plan Requirements for Municipal Solid Waste Landfills That Commenced Construction On or Before July 17, 2014 and Have Not Been Modified or Reconstructed Since July 17, 2014 
The Federal Plan implementing the 2016 Emission Guidelines and Compliance Times for Existing Municipal Solid Waste Landfills (40 CFR 60 Subpart Cf) was finalized on May 10, 2021.  Since MDEQ does not have an approved State Plan, Subpart OOO is in effect and enforceable solely by EPA Region 4 (until such time that MDEQ formally adopts the Federal Plan or EPA approves MDEQ’s State Plan).  
Since Canton Landfill’s current design capacity is less than 2.5 million megagrams per year and 2.5 million cubic meters, the facility was only required to submit the initial design capacity report until such time the landfill is modified to exceed the referenced thresholds. Should the Canton Landfill undergo an expansion, the landfill will become subject to the requirements of 40 CFR Part 60 – Subpart XXX, and the Federal Plan and State Plan will no longer apply. 

SPECIFIC APPLICABLE REQUIREMENTS

	Emission Point No.
	Pollutant
	Draft Permit Emission Limits
	Monitoring Requirements

	AA-001
	NMOCs
	34 Mg/yr NMOC emission threshold for control of landfill gas
	Determine NMOC emission rate on an annual basis, unless otherwise specified
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