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PERMIT REVIEW SUMMARY

Permit Writer:	Ryan Wigginton 				Date:	September 9, 2026
Company Name:	Utility Optimization Group LLC
Facility Location:	6917 Stennis Boulevard
Source Number:	1280-00049
County: 		Jackson

FACILITY DESCRIPTION
Utility Optimization Group, LLC, operates an existing manufacturing facility.  Operations at the site fall under SIC Codes 3443 (Fabricated Plate Work (Boiler Shops)) and 3498 (Fabricated Pipe and Pipe Fittings) as well as NAICS Codes 332313 (Plate Work Manufacturing) and 332996 (Fabricated Pipe and Pipe Fittings).  The facility receives steel and other materials to manufacture vessels, pipes, and other metal products.  Products are fabricated, cleaned, blasted, and coated based on design requirements or product specifications.  Major processes resulting in air emissions are painting/coating via spray guns in a building (Emission Point AA-001); indoor and outdoor abrasive blasting operations (Emission Point AA-002); metal fabrication operations such as welding, grinding, and other general metal working activities (Emission Point AA-003); and miscellaneous mobile equipment such as air compressors, hand-held metal working tools, blast cabinets, etc. (Emission Point AA-005).  The facility is an existing synthetic minor operating site for criteria pollutants and a synthetic minor source of hazardous air pollutants.

PROJECT/PERMIT ACTION DESCRIPTION
No changes are requested as a part of this permitting action.  Some permit conditions were modernized to reflect current permitting processes and more accurately reflect the Federal rules.  State fuel burning particulate matter (PM) standard was revised to only be applicable to the space heaters (Emission Point AA-009). The state fuel burning standard for sulfur dioxide (SO2) was also incorporated into the permit for this emission unit.

EMISSION SUMMARY
	Pollutant
	Potential-to-Emit (tons/year)

	PM10/PM2.5
	99.01

	SO2
	0.14

	NOX
	3.13

	CO
	1.8

	VOC
	99.01

	Total HAP
	24.01

	Individual HAP
	9.01


1Facility-wide emission limitation incorporated into the permit.

APPLICABLE/PROPOSED PERMIT LIMITATIONS

	Emission Point
	Pollutant/ Parameter
	Limitation/Standard
	Monitoring/Recordkeeping Requirement

	AA-100 (Facility-Wide)
	Opacity
	≤ 40% (from smoke)
	Method 9 and 22

	
	
	≤ 40%
	

	
	PM (filterable only)
	E = 4.1 × p0.67
	Margin of compliance is large.  No monitoring or recordkeeping proposed.

	
	Any Contaminant
	General Nuisance Provisions
	General state regulation.

	
	VOC
	≤ 99.0 tpy
	Monitor and record all VOC containing material

	
	PM10/PM2.5 (filterable + condensable)
	≤ 99.0 tpy
	Monitor and record material throughput to calculate PM emissions

	
	Individual HAP
	≤ 9.0 tpy
	Monitor and record all HAP containing material

	
	Total HAP
	≤ 24.0 tpy
	

	AA-009
	PM (filterable only)
	≤ 0.6 lb/MMBTU
	Margin of compliance is large.  No monitoring or recordkeeping proposed.

	
	SO2
	≤ 4.8 lb/MMBTU
	



NSPS APPLICABILITY
40 CFR 60, Subpart Kc/Kb/Ka, Standards of Performance for Petroleum Liquids and Volatile Organic Liquid Storage Vessels – these NSPS’s apply to tanks with various criteria for applicability including contents, size, and date constructed for each tank.  The tanks at the site are significantly smaller than the size thresholds for these subparts; therefore, the subpart does not apply.

40 CFR 60, Subpart IIII/JJJJ, Standards of Performance for Stationary Compression and Spark Ignition Internal Combustion Engines – these NSPS’s apply to engines.  The two (2) engines at the site associated with the air compressors are considered mobile sources; therefore, this subpart does not apply.

MACT APPLICABILITY
40 CFR 63, Subpart XXXXXX, National Emission Standards for Hazardous Air Pollutants Area Source Standards for Nine Metal Fabrication and Finishing Source Categories – this subpart applies to area sources of HAP that are primarily engaged in one of nine metal fabrication and finishing operations.  Utility Optimization’s operations fall under SIC codes 3443 and 3498. SIC Code 3433 is listed as an applicable source category on EPA’s Subpart XXXXXX guidance document.  Therefore, this subpart does apply.  The subpart has work practice standards for abrasive blasting, machining, grinding, polishing, and welding operations (Emission Points AA-002, AA-003, and AA-005).  The subpart also has standards for spray painting. The surface coating operations (Emission Point AA-001) do not utilize coatings that contain metal HAP (MFHAP); therefore, these standards are not applicable to operations at the site.  For the record, Conditions 4.6 and 4.7 in the previous permit were combined in this permitting action under Condition 4.5.

40 CFR 63, Subpart MMMM, National Emission Standards for Hazardous Air Pollutants for Surface Coating of Miscellaneous Metal Parts and Products – this subpart applies to metal coating operations at a major source of HAP.  This site is an area source of HAP; therefore, this subpart does not apply.

40 CFR 63, Subpart ZZZZ, National Emissions Standards for Hazardous Air Pollutants for Stationary Reciprocating Internal Combustion Engines – this subpart applies to engines.  This facility operates two (2) internal combustion engines for the air compressors; however, these units are mobile sources.  Therefore, this subpart does not apply.

40 CFR 63, Subpart HHHHHH, National Emission Standards for Hazardous Air Pollutants: Paint Stripping and Miscellaneous Surface Coating Operations at Area Sources – this subpart applies to area sources of HAP that engage in paint stripping using methylene chloride (MeCl), autobody refinishing of motor vehicles and mobile equipment, and spray application of coatings containing chromium (Cr), lead (Pb), manganese (mg), nickel (Ni), and/or cadmium (Cd).  The facility does not utilize methylene chloride, refinish motor vehicles or mobile equipment, or spray apply coatings containing any of the target MFHAP; therefore, this subpart does not apply.

PUBLIC PARTICIPATION
The 30-day public notice period began on September 30, 2026, when the notice was posted on MDEQ’s website and ends November 2, 2026 .
6244 PER20250001
6244 PER20250001
